Enable

Conf ter

vlan 10

name gestión

exit

interface range fa0/1-5

switchport mode Access vlan 10

exit

interface fa0/24

switchport mode access trunk

exit

running-config startup-config