Enable

Conf ter

vlan 10

name gestión

exit

interface range fa0/1-5

switchport mode Access vlan 10

exit

interface fa0/24

switchport mode access trunk

exit

running-config startup-config

router

int fa0/0.1

encapsulation dot1q 10

ip address tal

config int fa 0/0 no shut